# Package s3games.robot

- Class Summary
  Class | Description
  --- | ---
  Camera | Camera singleton is an object that communicates with the C++ application to retrieve the locations of the elements on the real board.
  CameraObjectType | Specifies the color (in HSV model) and size range for a particular element type and state as appears in the image frame seen from the camera.
  Robot | The main robot arm controller.
  RobotCmd | This class knows the details of the SSC-32 serial communication protocol, and translates the meaningful commands into low-level strings that are sent over the serial line to the SSC-32 servo controller
  RobotLocation | Represents a particular robot location - i.e.
  RobotSerialPort | RobotSerialPort class is responsible for communicating with the SSC-32 robot controller over the serial line.

- Enum Summary
  Enum | Description
  --- | ---
  RobotCmd.Command | list of available commands