# Packet switching

### From Wikipedia, the free encyclopedia.

In computer networking and telecommunications, packet switching is a communications paradigm in which packets (messages or fragments of messages) are individually routed between nodes, with no previously established communication path.

Packet switching was invented by Donald Davies and Paul Baran in the early 1960s. Some people claim that Leonard Kleinrock also invented packet switching, but Davies contested this prior to his death and pointed out that Kleinrock's research was actually in queueing theory, which is a key theoretical underpinning to packet switching. Kleinrock's published works nowhere mention breaking a user's message up into segments, and sending the segments through the network separately, which was the key innovation in Baran's and Davies' work.

A packet is a block of user data together with necessary address and administration information attached, to allow the network to deliver the data to the correct destination. One data connection will usually carry a stream of packets of data that will not necessarily be all routed the same way over the physical network.

Analogous to a physical packet sent through the post with the address written on the outside, this provides the information the network (the postal service) needs to get the packet to the correct destination.

Packets are routed to their destination through the most expedient route (as determined by some routing algorithm). Not all packets travelling between the same two hosts, even those from a single message, will necessarily follow the same route.

The destination computer reassembles the packets into their appropriate sequence. Packet switching is used to optimise the use of the bandwidth available in a network and to minimise the latency. Ethernet, X.25 and Frame relay are international standard layer 2 packet switching networks. Compare with ATM which uses cell relay instead of packet switching.

Notably, the Internet is a packet-switched network, running the Internet Protocol layer 3 protocol over a variety of other network technologies. Newer mobile phone technologies such as GPRS and i-mode also employ packet switching.

Also called connectionless. Opposite of circuit switched or connection-oriented networking, although technologies such as MPLS are beginning to blur the boundaries between the two.

[edit]

## See also

- Public switched data network
- Message switching
- ARPANET
- History of the Internet

[edit]

## Further reading

- Paul Baran, On Distributed Communications (http://www.rand.org/publications/RM/baran.list.html)
- Paul Baran, On Distributed Communications Networks (IEEE Transactions on Communications Systems, March 1964)
- Leonard Kleinrock, Information Flow in Large Communication Nets (http://www.lk.cs.ucla.edu/LK/Bib/REPORT/PhD/), (MIT, Cambridge, May 31, 1961) Proposal for a Ph.D. Thesis
- Leonard Kleinrock, Communication Nets: Stochastic Message Flow and Design (McGraw-Hill, 1964)
- Katie Hafner, Where Wizards Stay Up Late (Simon and Schuster, 1996)

[edit]

## External links

- Paul Baran and the Origins of the Internet (http://www.rand.org/about/history/baran.html)
- Leonard Kleinrock's Personal History/Biography (http://www.lk.cs.ucla.edu/LK/Inet/birth.html)
- Len Kleinrock on the Origins (http://www.computer.org/internet/v1n3/kleinrock9702.htm)
- The Internet Society History Page (http://www.isoc.org/internet/history/brief.shtml)
- Hobbes' Internet Timeline v7.0 (http://www.zakon.org/robert/internet/timeline/)
- VoIP - Packet Switching (http://www.voip.mn/packet-switching.html)

This article was originally based on material from the Free On-line Dictionary of Computing, which is licensed under the GFDL.

Retrieved from "http://en.wikipedia.org/wiki/Packet_switching"

Categories: Computer networks | Telecommunications

##### Views

- Article
- Discussion
- Edit this page
- History

##### Personal tools

- Create account / log in

##### Search

##### Toolbox

- What links here
- Related changes
- Special pages

##### In other languages

- Deutsch
- Suomi
- Italiano
- Norsk